REAR SCUFF PLATE REMOVAL/INSTALLATION

id091700801500

Rear Scuff Plate Inner

1. Pull the rear scuff plate inner upward while detaching tab A, detach clips B, pins C, and tab D, from the body, and then remove the rear scuff plate inner.

ac9uuw00000403

2. Install in the reverse order of removal.

Rear Scuff Plate Outer

1. Pull the rear scuff plate outer upward, detach clips A, tabs B, and pin C, from the body, and then remove the rear scuff plate outer.

ac9uuw00000404

2. Install in the reverse order of removal.