JACKING POSITIONS, VEHICLE LIFT (2 SUPPORTS) AND SAFETY STAND (RIGID RACK) POSITIONS

id000000800500

Jacking Positions

  Warning
  • Improperly jacking a vehicle is dangerous. The vehicle can slip off the jack and cause serious injury. Use only the correct front and rear jacking points and block the wheels.

• Use safety stands to support the vehicle after it has been lifted.

Front

  • Near the center or the front crossmember.

Rear

  • Near the center of the rear crossmember.
  • At the center of the rear differential.

ac9wzw00001017

Vehicle Lift and Safety Stand Positions

Front and rear

  Warning
  • When using an auto lift, if a vehicle is lifted under unstable conditions, the vehicle could fall off the lift while it is being lifted or during servicing, leading to serious injury or death and vehicle damage. Before lifting a vehicle with an auto lift, always adjust the height of the lift pads on the end of the arms and verify that the vehicle is at a level angle.

  Caution
  • For vehicles with side step molding, be careful not to damage the side step molding by hitting it with auto-lift arms or a safety stand.

  • Both sides of the vehicle, on side sills.

ac9wzw00000611