CAMSHAFT CONSTRUCTION [MZI-3.7]

id0110c5101300

• There is a camshaft sprocket positioning pin at the end of the camshaft, and a key groove in the camshaft sprocket. Mis-assembly can be prevented by aligning the positioning pin with the key groove when assembling.
• The detection unit for the camshaft position (CMP) sensor is at the intake port side camshaft.
• The groove for securing the No.1 cylinder TDC of the camshaft is provided at the top of the intake and exhaust camshaft.

ac9uun00000038