ON-BOARD DIAGNOSIS SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM) SIMULATION FUNCTION

id091400602100

Simulation Function

• The simulation function is used for optionally selecting simulation items of output parts preset in the keyless control module, and to operate them regardless of control.

ACTIVE COMMAND MODE TABLE

Command name | Output part name | Unit/Operation | Terminal
--- | --- | --- | ---
BZR_OUT | Keyless beeper | On/Off | 2K
BZR_INN | Interior buzzer (Instrument cluster) | On/Off | 3W, 3X
LNP_RED | Keyless warning light (red) | On/Off | 3W, 3X
LNP_GREEN | Keyless indicator light (green) | On/Off | 3W, 3X
DR_LOCK | All doors lock | Off/Lock | 3Q
DR_UNLOCK | All doors unlock | Off/Unlock | 3Q