MICROPHONE CONSTRUCTION/OPERATION

id092000100700

• Located in the map light.
• Recognize the voice entry.

L.H.D.

ac9wzn00000988

R.H.D.

ac9uun00000351

Terminal Layout and Signals

L.H.D.

Terminal | Signals
--- | ---
6-pin connector
| A | Mic (+)
B | Mic (-)
C | Mic B+
D | GND
E | Mic detect
F | —

R.H.D.

Terminal | Signals
--- | ---
6-pin connector
| A | Mic (+)
B | Mic (-)
C | Mic B+
D | GND
E | —
F | Mic detect