BRAKE FEATURES

id040000100200

Improved safety | • Intrusion minimizing brake pedal adopted • Large power brake unit (10.5 inch) adopted • ABS adopted • Electronic brakeforce distribution (EBD) control adopted • Electrical brake assist control has been adopted • Dynamic stability control (DSC)/Roll stability control (RSC) adopted
Improved braking force | • Large diameter front disc brakes adopted • Front brake caliper (two-piston type) adopted • Large diameter rear disc brakes adopted (Integrated with parking drum brake)
Improved serviceability | • Enhanced malfunction diagnosis system for use with Mazda Modular Diagnostic System (M-MDS) • Steering angle sensor that uses controller area network (CAN) adopted
Improved operability | • Foot-operated parking brake adopted
Size and weight reduction | • Integrated construction of the hydraulic unit (HU) and control module (CM) adopted for the DSC/RSC HU/CM
Improved brake pedal operability | • A master cylinder with smaller diameter long-stroke type has been adopted
Improved reliability | • Sophisticated Air Bag Sensor (SAS) control module integrating yaw rate, roll rate, and low-G (XY) sensors adopted • Specialized CAN communication adopted for communications between the SAS control module and the DSC/RSC HU/CM