PARKING BRAKE SWITCH INSPECTION

id041200800700

1. Disconnect the parking brake switch connector.

2. Verify that the continuity is as indicated in the table.

ampjjw00002631

  • If not as indicated in the table, replace the parking brake switch. (See PARKING BRAKE REMOVAL/INSTALLATION [2WD (L.H.D.)].) (See PARKING BRAKE REMOVAL/INSTALLATION [2WD (R.H.D.)].) (See PARKING BRAKE REMOVAL/INSTALLATION [4WD (L.H.D.)].) (See PARKING BRAKE REMOVAL/INSTALLATION [4WD (R.H.D.)].)

  acxuuw00001059