CLEARING FREEZE FRAME DATA [THEFT-DETERRENT SYSTEM]

id0902g7466200

1. Connect the M-MDS (IDS) to DLC-2.

ac9uuw00000452

2. After the vehicle is identified, select the following items from the initial screen of the M-MDS.

  • When using the IDS (laptop PC)
    1. Select the “Body”.
    2. Select the “VSM Service Functions”.

3. Then, select an item from the screen menu.

  (1) Select the “Clear FFD”.

4. Perform the procedure according to the directions on the screen.