REAR BUMPER DISASSEMBLY/ASSEMBLY

id091000800800

1. Disassemble in the order indicated in the table.

ac9wzw00000192

1 | Fastener A
2 | Bracket A
3 | Screw A
4 | Bracket B
5 | Screw B
6 | Rear reflector (See Reflector Removal Note)
7 | Nut
8 | Rear over fender lower (SeeRear Over Fender Lower Assembly Note)
9 | Insulator
10 | Rear bumper fascia
11 | Clip (R.H.D.)

2. Assemble in the reverse order of disassembly.

Reflector Removal Note

1. Pull off the reflector from the rear bumper in the direction and in the order as shown by the arrows.

ac9uuw00002271

Rear Over Fender Lower Assembly Note

1. Attach the rear over fender lower to the rear bumper fascia with nuts.

ac9uuw00001319

2. Use a soldering copper and thermally deform the tab in order to fasten the stiffening rib.