NO.8 CD PLAYER DOES NOT INDICATE THE MP3/WMA TITLE TEXT [CD PLAYER]

id0903k3992500

8 | CD player does not indicate the MP3/WMA title text
--- | ---
Possible DTC | Using the M-MDS | B1D19:71, B1188:64
Without using M-MDS (On-board diagnostic test mode) | 10:Er02, 10:Er07
Possible cause | • Defective CD-R/RW (e.g. dirty CD, scratch) • Conflict of ID tag version for CD-R/RW (MP3) • The number of characters of folder/audio file name in CD-R/RW exceeds the maximum number of characters • Improper encode in CD-R/RW • No title input in CD-R/RW • Input title text by 2-bytes characters • Audio unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | • Visually inspect the CD-R/RW. • Is there any dirt or scratch on the CD-R/RW? | Yes | Clean the disc or replace with the CD-R/RW known to be good.
No | Go to the next step.
2 | • Inspect the display the LCD. • Is the CD (other than MP3/WMA compatible) displayed on the LCD? | Yes | Go to the next step. (MP3)/Go to the step 4. (WMA)
No | Replace the audio panel. (See AUDIO UNIT REMOVAL/INSTALLATION.)
3 | • Inspect the ID tag version. • Is the ID tag correct? | Yes | Go to the next step.
No | Write the CD-R/RW with the correct ID tag version.
4 | • Is the title text input into the CD-R/RW? | Yes | Go to the next step.
No | Input the title text. Note • Do not input the title text by two-bytes character.
5 | • Inspect the encode for the folder and audio file name in the CD-R/RW. • Is the encode correct? | Yes | Go to the next step.
No | Use the correct encode.
6 | • Inspect the number of characters for the folder and audio file name. • Is the number of characters within the maximum number of characters? | Yes | Replace the audio unit. (See AUDIO UNIT REMOVAL/INSTALLATION.)
No | Input the folder and audio file name within the maximum number of characters.