LOAD LIMITER RETRACTOR CONSTRUCTION/OPERATION

id081100100300

1. Initial state

ac9wzn00000130

2. Pre-tensioner and ELR operation

ac9wzn00000327

When the vehicle has been subjected to an impact, the pre-tensioner or ELR activates, locking the belt and securing the passenger’s body.

3. Load limiter operation

ac9wzn00000132

After locking, if the force of impact transferred to the belt is strong enough to cause injury to the chest of the occupant, an adequate amount of belt is released to absorb the load applied to the chest.