DTC TABLE [HEADLIGHT AUTO LEVELING SYSTEM]

id0902i7347100

  Note
  • The headlight auto leveling warning light flashes in the following pattern when the headlight auto leveling system is normal.

  ac9wzw00001466

  • If the headlight auto leveling system has a malfunction, the headlight auto leveling warning light flashes in the following pattern and a DTC is output.

  ac9wzw00001486

  • All the detected DTCs are output repeatedly during DTC inspection.
  • If multiple DTCs are detected, the DTCs are output in the order from the lowest number.

DTC | DESCRIPTION | Reference
--- | --- | ---
Flashing pattern (Headlight auto leveling warning light)
11 |  | Auto leveling control module initial setting | (See DTC 11 [HEADLIGHT AUTO LEVELING SYSTEM].)
12 |  | Signals during front/rear auto leveling sensor initial setting | (See DTC 12 [HEADLIGHT AUTO LEVELING SYSTEM].)
21 |  | Rear auto leveling sensor signals | (See DTC 21 [HEADLIGHT AUTO LEVELING SYSTEM].)
22 |  | Front auto leveling sensor signals | (See DTC 22 [HEADLIGHT AUTO LEVELING SYSTEM].)
23 |  | Front /rear auto leveling sensor power supply | (See DTC 23 [HEADLIGHT AUTO LEVELING SYSTEM].)
24 |  | Front/rear auto leveling sensor pitch angles | (See DTC 24 [HEADLIGHT AUTO LEVELING SYSTEM].)
31 |  | Headlight leveling actuator signals | (See DTC 31 [HEADLIGHT AUTO LEVELING SYSTEM].)
41 |  | Auto leveling control module initial setting | (See DTC 41 [HEADLIGHT AUTO LEVELING SYSTEM].)