AUTOMATIC GEAR SHIFT CONTROL OUTLINE [AY6A-EL, AY6AX-EL]

id0517k3225700

• In automatic gear shift control, based on each gear shift pattern, shift solenoid A and shift solenoid B turn on or off and shift solenoid C, shift solenoid D, shift solenoid E, and shift solenoid F are operated linearly according to information that includes vehicle speed, accelerator pedal depressing amount, and brake signals.