RADIATOR CONSTRUCTION [MZI-3.7]

id0112d3142000

• A corrugated fin type radiator has been adopted.
• The radiator tanks are made of plastic and the core is made of aluminum for weight reduction.
• The down-flow direction of water inside the radiator causes air to bleed from the cooling system easier.
• Four mounting rubbers are utilized to decrease vibration.
• The radiator has an ATF oil cooler in the lower radiator tank.

ac9wzn00000663