AUTO LIGHT/WIPER CONTROL MODULE REMOVAL/INSTALLATION

id091900809000

  Note
  • Auto wiper system are integrated with the auto light/wiper control module.

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Remove the auto light/wiper control module. (See AUTO LIGHT/WIPER CONTROL MODULE REMOVAL/INSTALLATION.)

4. Install in the reverse order of removal.