AUDIO SYSTEM SPECIFICATIONS

id092000100400

Audio Unit

Item | Specification
--- | ---
Rated voltage | (V) | 12
Frequency band | AM | LW | (kHz) | 153—279
MW | (kHz) | 531—1602 (European specs.) 522—1629 (With AM frequency pitch: 9KHz pitch) 530—1620 (With AM frequency pitch: 5KHz pitch)
FM | (MHz) | 87.5—108
Audio amplifier maximum output power | (W) | With Bose®: 296 (External type audio amplifier) Without Bose®: 25×4
Output impedance | (ohm) | 3.6—4.6
Display* | Size | (in) | 5.8
Type |  | TFT (Thin Film Transistor); Full-color

Speaker

Item | Specification
--- | ---
Without Bose® | With Bose®
Front door speaker / Rear door speaker | Tweeter | Front door speaker | Rear door speaker | Front speaker / Rear speaker / Center speaker | Bass-box
Maximum input | (W) | 25 | 25 | 37 | 37 | 18.5 | 74
Impedance | (ohm) | 4 | 4 | 2 | 2 | 3.6 | 1
Size | (mm {in}) | 140×190 {5.5×7.5} | 30 {1.2} | 230 {9} | 165 {6.5} | 80 {3} | 370×420×150 {14.5×16.5×6}