TRANSMISSION/TRANSAXLE FEATURES

id050000302000

Automatic Transaxle [AY6A-EL, AY6AX-EL]

Superior shift quality | • Self learning control has been adopted. • Centrifugal hydraulic pressure cancel clutch has been adopted. • Garage shift control has been adopted. • Engine-transaxle total control system has been adopted.
High efficiency | • Slip control system has been adopted.
Improved reliability | • The TR switch integral type TCM has been adopted.
Improved driveability | • A control feature for climbing/descending hills has been adopted, improving driveability when climbing/descending.
Improved marketability | • The Sport AT has been adopted.
Mis-shift prevention | • Reverse control has been adopted. • A key interlock system has been adopted. • A shift-lock system has been adopted.