FRONT FRAME (REAR) INSTALLATION [PANEL REPLACEMENT]

id098008742600

1. When installing new parts, measure and adjust the body as necessary to conform with standard dimensions.

2. Drill holes for the plug welding before installing the new parts.

3. Install the front frame rear component.

am8rrb00000103

4. After temporarily installing new parts, make sure the related parts fit properly.

5. Install the torque box.

am8rrb00000104