GLOBAL POSITIONING SYSTEM (GPS) ANTENNA REMOVAL/INSTALLATION

id092000801500

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (2) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (3) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (4) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (5) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

3. Remove in the order indicated in the table.

ac9wzw00000769

1 | Connector
2 | Screw
3 | Clip
4 | GPS antenna

4. Install in the reverse order of removal.