PARKING SENSOR CONTROL MODULE REMOVAL/INSTALLATION

id092200023500

1. Disconnect the negative battery cable.

2. Remove the trunk box. (See TRUNK BOX REMOVAL/INSTALLATION.)

3. Disconnect the connector.

ac9wzw00002674

4. Remove the nuts.

5. Pull the clip in the direction of the arrow (2) shown in the figure while pressing the clip in the direction of the arrow (1) shown in the figure, detach the clip and parking sensor control module bracket, and then remove the clip from the parking sensor control module bracket.

ac9wzw00002735

6. Install in the reverse order of removal.