THEFT-DETERRENT SYSTEM OUTLINE [WITHOUT INTRUDER SENSOR]

id0914005990b8

• The theft-deterrent system includes sound and light alarms that activate when the hood, the liftgate, or a door is opened by means other than the ignition key or the transmitter. The turn lights flash and the horn sounds.
• When the ignition key is inserted into the door and turned to unlock or the transmitter unlock button is pressed, the alarms stop.