CABIN CONSTRUCTION

id091000100700

• An impact dispersing three-fork structure that disperses a collision impact into three directions has been adopted.
• A distribution of reinforcement to the floor, side frames, and roof employing an H-shaped structure to reinforce each joint has been adopted. the combination of three points to each floor, side frames, and roof surface provide the strong triple H-shaped structure.
• Suppression of cabin torsion while driving, and steering performance has been improved.

ac9uun00000510