Bluetooth SYSTEM CONSTRUCTION

id092000833700

• Consists of the following parts.

ac9wzn00000460

• Communication between the Bluetooth-enabled device and the Bluetooth unit is performed via radio waves. The frequency range is 2.4 GHz, and transmission is possible within an approx. 10 m (32 ft) area.
• Transmission between the Bluetooth unit, the vehicle’s audio and the information display is performed via the CAN system.
• The vehicle’s audio outputs the signals from the Bluetooth unit to the audio amplifier.
• The vehicle’s microphone is connected to the Bluetooth unit. The Bluetooth unit sends the voice spoken into the vehicle’s microphone to the Bluetooth-enabled device.