DTC 41 [HEADLIGHT AUTO LEVELING SYSTEM]

id0902i7404200

Description

• Auto leveling system initial setting

Detection Condition

• Auto leveling control module initial setting value write abnormal

Possible Cause

• Auto leveling system initial setting disabled
• Auto leveling control module malfunction

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | PERFORM AUTO LEVELING SYSTEM INITIAL SETTING • Perform the auto leveling system initial setting. (See AUTO LEVELING SYSTEM INITIALIZATION.) • Perform the headlight auto leveling system DTC inspection. (See DTC INSPECTION [HEADLIGHT AUTO LEVELING SYSTEM].) • Is DTC 41 displayed? | Yes | Replace the auto leveling control module. (See AUTO LEVELING CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.