WINDSHIELD WASHER NOZZLE REMOVAL/INSTALLATION

id091900802000

1. Remove the windshield wiper arm and blade. (See WINDSHIELD WIPER ARM AND BLADE REMOVAL/INSTALLATION.)

2. Remove the cowl grille. (See COWL GRILLE REMOVAL/INSTALLATION.)

3. Remove the windshield washer hose from the windshield washer nozzle.

4. Squeeze the tabs of the windshield washer nozzle.

5. Pull the windshield washer nozzle out to remove it.

ac9wzw00001603

6. Install in the reverse order of removal.