DASHBOARD UNDER COVER REMOVAL/INSTALLATION

id091700807200

Driver Side

1. Remove the fasteners.

ac9uuw00000367

2. Detach tab A and hook by pulling them in the direction of the arrow.

3. Remove the dashboard under cover.

4. Install in the reverse order of removal.

Passenger Side

1. Insert fingers into the service hole and detach clips A and pin B and hooks by pulling it in the direction of the arrow.

ac9uuw00000368

2. Remove the dashboard under cover.

3. Install in the reverse order of removal.