OVER FENDER REMOVAL/INSTALLATION

id091600820100

Front

1. Remove the fasteners.

ac9uuw00000724

2. Remove the clips A.

3. Remove the clip B.

4. Remove the clip C.

5. Remove the front over fender.

6. Install in the reverse order of removal.

Rear

1. Remove the fastener.

ac9uuw00000725

2. Remove the clips A.

3. Remove the clips B.

4. Remove the clip C.

5. Remove the rear over fender.

6. Install in the reverse order of removal.