SOLAR RADIATION SENSOR REMOVAL/INSTALLATION

id074000802800

1. Disconnect the negative battery cable.

2. Remove the cover from the dashboard using a flathead screwdriver wrapped with protective tape.

3. Detach the solar radiation sensor connector tab in the position shown in the figure and disconnect the solar radiation sensor connector.

4. Press the solar radiation sensor tab and remove the solar radiation sensor from the cover.

ac9wzw00002801

5. Install in the reverse order of removal.