BLIND SPOT MONITORING (BSM) INDICATOR LIGHT FUNCTION [BLIND SPOT MONITORING (BSM) CONTROL MODULE CONNECTOR 8-PIN TYPE]

id0922009983e1

• Illuminates when a vehicle enters the alert area to alert the driver.
• Flashes if the turn signal lever is operated to the side where a vehicle has entered the alert area and the BSM indicator light has illuminated in the outer mirror glass to warn the driver.

ac9wzn00000894