FUEL-FILLER LID OPENER REMOVAL/INSTALLATION

id091400804700

1. When removing the fuel-filler lid opener, perform the following procedure:

  (1) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (2) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (3) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (4) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (5) Rear scuff plate inner (Driver side) (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (6) Third-row seat belt lower anchor installation bolt (Driver side) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (7) Trunk side trim (Driver side) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

2. When removing the fuel-filler lid opener cable, perform the following procedure:

  (1) Front scuff plate inner (Driver side) (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (2) Rear scuff plate inner (Driver side) (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (4) B-pillar lower trim (Driver side) (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (5) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (6) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (7) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (8) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (9) Third-row seat belt lower anchor installation bolt (Driver side) (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (10) Trunk side trim (Driver side) (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

3. Remove the fuel-filler lid release cover in the direction of the arrow. (L.H.D.)

ac9uuw00002150

4. Slightly bend back the floor covering.

5. Remove in the order indicated in the table.

6. Install in the reverse order of removal.

R.H.D.

ac9wzw00000635

1 | Lift spring
2 | Fuel-filler lid opener
3 | Fuel-filler lid release lever
4 | Fuel-filler lid opener cable

L.H.D.

ac9uuw00002151

1 | Lift spring
2 | Fuel-filler lid opener
3 | Bolt
4 | Fastener
5 | Fuel-filler lid release lever
6 | Fuel-filler lid opener cable