CABIN SIDE FRAME STRAIGHT-LINE DIMENSIONS [DIMENSIONS]

id098010743600

ac9uub00000009

ac9uub00000010

ac9uub00000011

Point symbol | Designation | Hole diameter or bolt or nut size mm {in}
--- | --- | ---
A | Front side frame (outer) datum slot | 12 x 18 {0.47 x 0.71}
B | Front door hinge installation hole | φ12 {0.47}
C | Front door hinge installation hole | φ12 {0.47}
D | Side frame (outer) notch | -
E | Side frame (outer) projection location | -
F | Rear door hinge installation hole | φ12 {0.47}
G | Rear door hinge installation hole | φ12 {0.47}
H | Side frame (outer) projection location | -
I | Side frame (outer) notch | -
J | Quarter window glass installation hole | φ8 {0.31}
K | Rear door switch installation hole | φ4.5 {0.18}
L | Side frame (outer) square hole | 9 x 9 {0.35 x 0.35}