ENGINE CONTROL SYSTEM OUTLINE [MZI-3.7]

id0140c3100100

Features

Improved driveability | • Drive-by-wire control adopted • Fuel injection control adopted • Fuel pump control adopted
Improved emission performance | • Variable valve timing control adopted • A heater element is integrated with the A/F sensor and HO2S • All range sensor has been adopted for the A/F sensor
Improved fuel economy | • A drive-by-wire control (idle air control) has been adopted which contributes to lower fuel consumption
Wiring harness simplification | • CAN adopted

Specification

Item | Specification
--- | ---
PSP switch | Hydraulic pressure
CHT sensor | Thermistor
MAF sensor | Hot-wire
IAT sensor (Inside MAF sensor) | Thermistor
TP sensor | Potentiometer type
CKP sensor | Pickup type
CMP sensor | Pickup type
A/F sensor | Zirconia element (All range)
HO2S | Zirconia element (Stoichiometric)