ON-BOARD DIAGNOSTIC SYSTEM OUTLINE [Bluetooth SYSTEM (HANDS-FREE TELEPHONE (HF/TEL) SYSTEM)]

id0920001017a9

• The Bluetooth system (hands-free telephone (HF/TEL) system has an on-board diagnostic function and diagnostic assist function to facilitate Bluetooth system (hands-free telephone (HF/TEL) system diagnosis.
• The on-board diagnostic function consists of the following functions: A malfunction detection function, which detects overall malfunctions in the Bluetooth system (hands-free telephone (HF/TEL) system-related parts; a memory function, which stores detected DTCs; and a display function, which indicates system malfunctions via a DTC display.
• The diagnostic assist function enables verification of the connection condition of the Bluetooth system (hands-free telephone (HF/TEL) system related parts and their specification. The password for the Bluetooth system (hands-free telephone (HF/TEL) system), which is set by the user, can also be reset.