SECOND-ROW SEAT DISASSEMBLY/ASSEMBLY

id091300802600

LH

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

ac9wzw00002479

1 | Recliner lever
2 | Lift lever
3 | Hinge cover
4 | Knuckle upper cover
5 | Seat back board
6 | Armrest bracket
7 | Armrest
8 | Seat back trim
9 | Seat back pad
10 | Headrest
11 | Pole guide
12 | Seat back frame
13 | Seat under bracket cover
14 | Second-row buckle
15 | Slide adjuster cover
16 | Side cover
17 | Seat cushion trim
18 | Seat cushion pad
19 | Seat cushion frame
20 | Slide adjuster

RH

ac9wzw00002480

1 | Second-row buckle
2 | Recliner lever
3 | Lift lever
4 | Hinge cover
5 | Knuckle upper cover
6 | Seat back board
7 | Seat back trim
8 | Seat back pad
9 | Headrest
10 | Pole guide
11 | Seat back frame
12 | Seat under bracket cover
13 | Slide adjuster cover
14 | Side cover
15 | Seat cushion trim
16 | Seat cushion pad
17 | Seat cushion frame
18 | Slide adjuster