SHIFT SOLENOID A, B OUTLINE [AY6A-EL, AY6AX-EL]

id0517k3224800

• Shift solenoid A, B is installed on the front valve body. The solenoids turn ON and OFF in response to signals output from the TCM. According to the ON or OFF status of shift solenoid A or shift solenoid B, the 1st gear engine brake operates or a gear shift occurs. As a fail-safe function, if any shift solenoid abnormality occurs, the TCM will disable the current to the solenoids.

ac9uun00000790