STEERING GEAR AND LINKAGE CONSTRUCTION

id061400100600

• A size and weight reduced rack and pinion system steering gear has been adopted.
• Heightened support rigidity has been achieved due to the integration of the steering gear mounts and gear housing, improving response and steering stability.
• A check valve equipped on the power steering fluid intake port (pressure side) of some models prevents the power steering fluid from flowing back as a result of road surface resistance.

ac9wzn00000228

ac9wzn00000229