ON-BOARD DIAGNOSIS SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM) PID/DATA MONITOR FUNCTION

id091400601800

PID name (definition) | Data contents | Unit/Operation
--- | --- | ---
DTC_CNT | Number of continuous DTCs | −
RPM | Engine speed | RPM
VSS | Vehicle speed | KPH
VPWR | Supply voltage | V
NUMCARD | Number of programmed card keys | −
NUMKEY | Number of programmed key ID numbers | −
DRSW_D | Door switch (driver’s door) | CLOSE/OPEN
DRSW_ALL | Door switch (except driver’s door) | CLOSE/OPEN
REQ_SW_P | Request switch (right side door) | On/Off
REQ_SW_D | Request switch (left side door) | On/Off
REQ_SW_BK | Request switch (liftgate) | On/Off
LOCK_SW_D | Door lock-link switch (driver’s side) | On/Off
IMMOBI | Immobilizer system equipped or not | On/Off
TR/LG_SW | Trunk compartment light switch | CLOSE/OPEN
IG_KEY_IN | Key reminder switch | Key-In/Key-Out
IG_SW_ST | Ignition switch (Push switch) | Pushed/Not Pushed
BUZZER | Keyless beeper | On/Off
PWR_IG1 | Power supply (IG1) | On/Off
PWR_ACC | Power supply (ACC) | On/Off