ANTENNA FEEDER NO.2 REMOVAL/INSTALLATION

id092000812300

1. Disconnect the negative battery cable.

2. Partially peel back the seaming welt.

3. Remove the following parts:

  (1) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

  (2) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (3) Front side trim (RH) (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (4) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (5) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (6) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (7) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (8) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (9) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (10) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (11) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (12) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (13) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (14) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION)

  (15) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (16) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (17) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (18) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (19) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (20) Intruder sensor (with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

  (21) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (22) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (23) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

  (24) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

4. Disconnect the antenna feeder No.1.

L.H.D.

ac9wzw00001077

R.H.D.

ac9wzw00001078

5. Remove the clips A and B.

6. Remove the clips C, D and E.

Without sunroof

ac9wzw00001079

With sunroof

ac9wzw00001080

7. Remove the clips F.

ac9wzw00001081

8. Remove the bolt.

ac9wzw00001082

9. Disconnect the connector.

10. Remove in the antenna feeder No.2.

11. Install in the reverse order of removal.