DTC U0300:00, U2100:00, [THEFT-DETERRENT SYSTEM]

id0902g7850600

Detection Condition

• Possible configuration error

Possible Causes

• Configuration has not been correctly performed for some reason
• Theft-deterrent control module malfunction

Diagnostic Procedure

Step | Inspection | Action
--- | --- | ---
1 | VERIFY DTCs • Clear DTCs using the M-MDS. (See CLEARING DTC [THEFT-DETERRENT SYSTEM].) • Verify DTCs using the M-MDS. (See DTC INSPECTION [THEFT-DETERRENT SYSTEM].) • Is DTC U0300:00 or U2100:00 displayed? | Yes | Replace the theft-deterrent system control module. (See THEFT-DETERRENT CONTROL MODULE REMOVAL/INSTALLATION.)
No | DTC troubleshooting completed.