THEFT-DETERRENT CONTROL MODULE REMOVAL/INSTALLATION

id091400820800

1. Disconnect the negative battery cable.

2. Remove the following parts:

  (1) Dashboard under cover (Passenger side) (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (2) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

3. Remove the nut.

ac9wzw00001785

4. Remove the connector.

5. Remove the theft-deterrent control module.

6. Install in the reverse order of removal.