REAR SHOCK ABSORBER REMOVAL/INSTALLATION

id021400801300

1. Remove the trunk side trim. (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

2. Support the rear lower arm using a garage jack.

ampjjw00000888

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

ac9uuw00002796

1 | Nut
2 | Retainer
3 | Upper rubber bushing
4 | Bolt and nut (shock absorber lower side)
5 | Lower rubber bushing
6 | Retainer
7 | Rear shock absorber