PARKING SENSOR BUZZER REMOVAL/INSTALLATION

id092200023900

1. Disconnect the negative battery cable.

2. Remove the dashboard under cover (Driver side). (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

3. Disconnect the connector.

ac9wzw00002677

4. Pull out the rear parking sensor buzzer in the direction of arrow (2) shown in the figure while pressing the clip in the direction of arrow (1) shown in the figure and remove the rear parking sensor buzzer.

5. Install in the reverse order of removal.