CLEARING DTC [ADVANCED KEYLESS ENTRY AND START SYSTEM]

id09021g400300

1. Connect the M-MDS to the DLC-2.

L.H.D.

ac9uuw00000633

R.H.D.

ac9wzw00000487

2. After the vehicle is identified, select the following items from the initialization screen of the M-MDS.

  1. Select “Self Test”.
  2. Select “Modules”.
  3. Select “RKE”.

3. Verify the DTC according to the directions on the screen.

4. Press the clear button on the DTC screen to clear the DTC.

5. Verify that no DTCs are displayed.