FRONT DRAIN HOSE INSTALLATION

id091500801400

  Caution
  • If the front drain hose is pinched or bent anywhere, the water in the hose may not discharge and enter the inside of the vehicle. During and after installation of the trims and the headliner, always make sure there is no interference with the front drain hose. Fix any problem if found.

1. Apply soapy water to the front drain hose inserting area.

2. Insert one end (the wider end) of the front drain hose into the sunroof frame.

3. Install the front drain hose to the clips, parallel to the pillar and free of slack.

4. Insert the front drain hose joint into the hinge pillar inner hole.

5. Install the following parts:

  (1) Dashboard (See DASHBOARD REMOVAL/INSTALLATION.)

  (2) Side panel (See SIDE PANEL REMOVAL/INSTALLATION.)

  (3) Steering shaft (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (4) Car-navigation unit (vehicles with car-navigation system) (See CAR-NAVIGATION UNIT REMOVAL/INSTALLATION.)

  (5) Audio unit (vehicles with audio system) (See AUDIO UNIT REMOVAL/INSTALLATION.)

  (6) Instrument cluster (See INSTRUMENT CLUSTER REMOVAL/INSTALLATION.)

  (7) Meter hood (See METER HOOD REMOVAL/INSTALLATION.)

  (8) Center panel (See CENTER PANEL REMOVAL/INSTALLATION.)

  (9) Combination switch (See COMBINATION SWITCH REMOVAL/INSTALLATION.)

  (10) Steering wheel (See STEERING WHEEL AND COLUMN REMOVAL/INSTALLATION.)

  (11) Driver-side air bag module (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

  (12) Column cover (See COLUMN COVER REMOVAL/INSTALLATION.)

  (13) Lower panel (See LOWER PANEL REMOVAL/INSTALLATION.)

  (14) Fuel-filler lid release lever (R.H.D.) (See FUEL-FILLER LID OPENER REMOVAL/INSTALLATION.)

  (15) Bonnet release lever (See BONNET REMOVAL/INSTALLATION.)

  (16) Glove compartment (See GLOVE COMPARTMENT REMOVAL/INSTALLATION.)

  (17) Front side trim (See FRONT SIDE TRIM REMOVAL/INSTALLATION.)

  (18) Console (See CONSOLE REMOVAL/INSTALLATION.)

  (19) Console cover (See CONSOLE COVER REMOVAL/INSTALLATION.)

  (20) Console panel (See CONSOLE PANEL REMOVAL/INSTALLATION.)

  (21) Side wall (See SIDE WALL REMOVAL/INSTALLATION.)

  (22) Dashboard under cover (See DASHBOARD UNDER COVER REMOVAL/INSTALLATION.)

  (23) Front console box (See FRONT CONSOLE BOX REMOVAL/INSTALLATION.)

  (24) Indicator panel (See INDICATOR PANEL REMOVAL/INSTALLATION.)

  (25) Front console box mat (See FRONT CONSOLE BOX MAT REMOVAL/INSTALLATION.)

  (26) Decoration panel (See DECORATION PANEL REMOVAL/INSTALLATION.)

  (27) Headliner (See HEADLINER REMOVAL/INSTALLATION.)

  (28) Assist handle (See ASSIST HANDLE REMOVAL/INSTALLATION.)

  (29) Sunvisor (See SUNVISOR REMOVAL/INSTALLATION.)

  (30) Front map light (See FRONT MAP LIGHT REMOVAL/INSTALLATION.)

  (31) Intruder sensor (vehicles with intruder sensor) (See INTRUDER SENSOR REMOVAL/INSTALLATION.)

  (32) D-pillar trim (See D-PILLAR TRIM REMOVAL/INSTALLATION.)

  (33) Third-row seat belt upper anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (34) C-pillar trim (See C-PILLAR TRIM REMOVAL/INSTALLATION.)

  (35) Second-row seat belt upper anchor installation bolt (See SECOND-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (36) Roof side trim (See ROOF SIDE TRIM REMOVAL/INSTALLATION.)

  (37) Trunk side trim (See TRUNK SIDE TRIM REMOVAL/INSTALLATION.)

  (38) Third-row seat belt lower anchor installation bolt (See THIRD-ROW SEAT BELT REMOVAL/INSTALLATION.)

  (39) Third-row seat (See THIRD-ROW SEAT REMOVAL/INSTALLATION.)

  (40) Trunk end trim (See TRUNK END TRIM REMOVAL/INSTALLATION.)

  (41) Seat side box (See SEAT SIDE BOX REMOVAL/INSTALLATION.)

  (42) Trunk box (See TRUNK BOX REMOVAL/INSTALLATION.)

  (43) B-pillar upper trim (See B-PILLAR UPPER TRIM REMOVAL/INSTALLATION.)

  (44) Front seat belt upper anchor installation bolt (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (45) B-pillar lower trim (See B-PILLAR LOWER TRIM REMOVAL/INSTALLATION.)

  (46) Front seat belt lower anchor installation bolt (Driver side) (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  (47) Rear scuff plate inner (See REAR SCUFF PLATE REMOVAL/INSTALLATION.)

  (48) Front scuff plate inner (See FRONT SCUFF PLATE REMOVAL/INSTALLATION.)

  (49) A-pillar trim (See A-PILLAR TRIM REMOVAL/INSTALLATION.)

6. Install the seaming welt.