MASTER CYLINDER CONSTRUCTION

id041100100700

• With the adoption of the master cylinder having a long stroke and small diameter (22.2 mm {0.874 in}), brake pedal operability has been improved.
• Except for the reserve tank, the master cylinder cannot be disassembled. Therefore, if there is any malfunction in the interior of the master cylinder, replace the cylinder component without disassembling.

ac9wzn00000617