BATTERY REMOVAL/INSTALLATION [MZI-3.7]

id0117d2800500

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

ac9wzw00002129

1 | Negative battery cable
2 | Positive battery cable
3 | Battery clamp
4 | Battery box (See Battery Box Installation Note.)
5 | Battery
6 | Battery tray

Battery Box Installation Note

1. Install the battery box so that the side with the notch points toward the front fender (LH).

ac9wzw00002130