DTC TABLE [POSITION MEMORY CONTROL SYSTEM]

id0902z8998400

DTC | Description | Page
--- | --- | ---
M-MDS display
U3003 16 | Battery voltage low | DTC U3003:16 [POSITION MEMORY CONTROL SYSTEM]
U0001:88 | CAN system communication error | FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (L.H.D.)] FOREWORD [MULTIPLEX COMMUNICATION SYSTEM (R.H.D.)]
U0100:00 | Communication error to PCM
U0101:00 | Communication error to TCM
U0121:00 | Communication error to DSC/RSC HU/CM
U0140:00 | Communication error to BCM
U0155:88 | Communication error to instrument cluster
U0431 68 | Invalid data received from body control module “A“ | DTC U0431:68 [POSITION MEMORY CONTROL SYSTEM]
B1B87 13 | Rear tilt motor speed/position sensor communication fault | DTC B1B87:13 [POSITION MEMORY CONTROL SYSTEM]
B1B89 13 | Slide motor speed/position sensor communication fault | DTC B1B89:13 [POSITION MEMORY CONTROL SYSTEM]
B1B91 13 | Front tilt motor speed/position sensor communication fault | DTC B1B91:13 [POSITION MEMORY CONTROL SYSTEM]
B1B93 13 | Recline motor speed/position sensor communication fault | DTC B1B93:13 [POSITION MEMORY CONTROL SYSTEM]
B1377 13 | Left mirror horizontal position sensor communication fault | DTC B1377:13 [POSITION MEMORY CONTROL SYSTEM]
B1386 13 | Right mirror horizontal position sensor communication fault | DTC B1386:13 [POSITION MEMORY CONTROL SYSTEM]
B1387 13 | Left mirror vertical position sensor communication fault | DTC B1387:13 [POSITION MEMORY CONTROL SYSTEM]
B1388 13 | Right mirror vertical position sensor communication fault | DTC B1388:13 [POSITION MEMORY CONTROL SYSTEM]