SYMPTOM TROUBLESHOOTING CHART [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]

id0903j4805600

No. | Malfunction symptom
--- | ---
1 | No.1 THE AUTO OPEN/CLOSE FUNCTION ON THE DRIVER'S SIDE POWER WINDOW IS INOPERATIVE [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]
2 | No.2 THE DRIVER'S SIDE POWER WINDOW IS INOPERATIVE [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]
3 | No.3 ALL POWER WINDOWS OTHER THAN DRIVER'S SIDE DO NOT OPERATE USING THE POWER WINDOW SUBSWITCH [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]
4 | No.4 ALL POWER WINDOWS OTHER THAN DRIVER'S SIDE DO NOT OPERATE USING THE POWER WINDOW MAIN SWITCH [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]
5 | No.5 ALL POWER WINDOWS ARE INOPERATIVE [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]
6 | No.6 DOOR GLASS REVERSES EVEN THOUGH THE GLASS DOES NOT ENCOUNTER A FOREIGN OBJECT WHILE IT IS MOVING UP IN AUTOMATIC MODE [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]
7 | No.7 ABNORMAL NOISE WHILE THE DOOR GLASS IS OPENING OR CLOSING [POWER WINDOW SYSTEMS (WITHOUT EXTERIOR OPEN/CLOSE FUNCTION)]