ON-BOARD DIAGNOSTIC SYSTEM DIAGNOSTIC DATA MEMORY FUNCTION [AY6A-EL, AY6AX-EL]

id0502k1280300

• The on-board diagnostic system data memory function records/erases the following diagnostic data.

  ― Number of DTCs
  ― DTCs
  ― Pending code
  ― Freeze frame data

• The conditions for recording/erasing diagnostic data are determined by the number of drive cycles set for each DTC.
• Using the memory deletion function of the Mazda Modular Diagnostic System (M-MDS), diagnostic data can be deleted.