DTC TABLE [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]

id09021h347100

DTC | Detection condition | Page
--- | --- | ---
Security light flashing pattern | M-MDS display*1
Keyless control module | PCM*2 | PCM*3
11 |  | B1681 | P1260 | P1260:00 | No detected communication with the coil antenna | SECURITY LIGHT: 11, DTC: B1681/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
12 |  | B2103 | P1260 | P1260:00 | Coil antenna malfunction | SECURITY LIGHT: 12, DTC: B2103/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
13 |  | B1600 | P1260 | P1260:00 | The key ID number data cannot be read | SECURITY LIGHT: 13, DTC: B1600/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
B2431 | P1260 | P1260:00 | Key ID number registration error | SECURITY LIGHT: 13, DTC: B2431/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
14 |  | B1602 | P1260 | P1260:00 | The keyless control module cannot read key ID number data normally | SECURITY LIGHT: 14, DTC: B1602/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
15 |  | B1601 | P1260 | P1260:00 | The keyless control module has detected unregistered key ID number | SECURITY LIGHT: 15, DTC: B1601/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
16 |  | U2510 | P1260 | P1260:00 | Communication error between the keyless control module and the PCM (mismatched conditions) | SECURITY LIGHT: 16, DTC: U2510/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
21 |  | B1213 | P1260 | P1260:00 | Only one key ID number is registered | SECURITY LIGHT: 21, DTC: B1213/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
22 |  | B2141 | P1260 | P1260:00 | Communication error between the keyless control module and the PCM (data transfer error) | SECURITY LIGHT: 22, DTC: B2141/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
23 |  | B2139 | P1260 | P1260:00 | ID number data in the PCM and the keyless control module do not match | SECURITY LIGHT: 23, DTC: B2139/P1260/P1260:00 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]
Not illuminated | B1342 | - | - | Keyless control module malfunction | DTC B1342 [IMMOBILIZER SYSTEM (ADVANCED KEYLESS ENTRY AND START SYSTEM)]

*1 :The letters at the beginning of each DTC are only displayed when using the M-MDS, and refer to the following: B= Body system, P= Powertrain system, U= Network communication system.
*2 :PCM connector (2 types)
*3 :PCM connector (3 types)